
ADEY® MC5™ and MC40+™ System Treatment Formulas: Innovative solutions that combat black sludge 

[bookmark: _GoBack]The two new products are part of ADEY’s Best Practice® approach to prolonging the life and efficiency of hydronic heating systems.
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Description automatically generated]Wilmington, DE (November 9, 2022) — ADEY, a U.K- based company whose pioneering MagnaClean CMX® range was recently rolled out in the United States and Canada, is introducing a line of innovative, concentrated system treatment formulas, designed to clean and protect older hydronic heating systems and retrofit installs. MC5™ Cleaner and MC40+™ De-scaler serve different purposes, but both were created to combat a frequently overlooked enemy of untreated hydronic heating systems – black sludge.
The MC40+ Hydronic Heating System Cleaner & De-scaler is a high-strength powdered chemical, specially designed to restore existing boiler systems by removing lime-scale deposits, calcium and magnetite. Rapid-performing MC40+ delivers an advanced clean, with a highly concentrated formula, in as little as one hour. It even comes with neutralizer packets to provide extra peace of mind if there is concern over residues being left in the system.
The second, MC5 Hydronic RAPIDFLUSH System Cleaner, is a high-performance, advanced-strength product, designed to work with ADEY’s award-winning MagnaCleanse® flushing unit. Together, they effectively remove sludge, debris, and scale while delivering exceptional cleaning results quickly.
Key features summary
MC40+: 
· Specifically designed to remove heavy lime-scale and calcium deposits from older systems with known water-quality issues or plugged components, such as heat exchangers.
· Preferred option to clean and drain the system quickly.
· Faster-acting, with a working time range of one to four hours. 
· Residential only – treats 33 gallons.
MC5: 
· Designed for flushing; works best with ADEY’s MagnaCleanse flushing unit.
· Faster-acting than the MC3+® but provides more time than the MC40+. Whether old or new, if the system is to be flushed on the same day that it is cleaned, this is the preferred cleaner option.
· Working time range: from a minimum of 1 hour to a maximum of 7 days.
· Residential size only, treating 26 gallons.
-more on next page-
For more information on the ADEY Treatment Formulas, please visit: https://www.adey.com/us.
For more information on the full line of ADEY filters and other Best Practice System Process solutions, visit adey.com/us. You can also phone +1 412 406 8292 or e-mail info@adeyusa.com.
For editorial assistance, contact John O’Reilly or Payton Meyers at GreenHouse Digital + PR, 15255 South 94th Avenue, Suite 500, Orland Park, IL 60462; tel.: 708.428.6385; e-mails: john@greenhousedigitalpr.com; payton@greenhousedigitalpr.com.

ADEY Innovation Ltd. is headquartered in Stonehouse, England, and has sales offices throughout the United Kingdom and Europe. U.S. operations are based in Wilmington, DE.
ADEY® is the industry-leading name in magnetic filtration, delivering Best Practice™ maintenance and protection for domestic and commercial hydronic heating systems. Best Practice heating system protection is a five-step process using products engineered to ensure maximum efficiency in hydronic heating systems. ADEY’s MagnaClean® filters are the best-selling brand in the U.K. with more than three million installed throughout Europe. Tens of thousands are fitted monthly, making it the leading filter for installers and homeowners. ADEY  filters also help protect the environment by reducing carbon emissions. ADEY also manufactures a growing range of premium quality chemicals developed in the U.K. at ADEY’s own accredited laboratory.
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